Rev – to Rev A differences

Schematic

Connected Reset\_N to +3.3V to make reset not active

Changed R6 from 300k to 100k as 300k is incorrect value

Changed R7 from 499k to 470k no real reason apart from that was the value used

Changed C4 from 15uF to 22uF as that was the value available when used

Changed R1 from 10k to 0R as needs to be 0R so programmer can supply voltage to Vcc

Added X9 to make Vout connection easier

Changed C5 from 15uF to 22uF as that was the value available when populating board